Connecting to Projectors over the network in the NETbuilder Manchester office

Below are listed the steps for connecting to a projector over the network in the Manchester office. NOTE: The Interactive capabilities of the projector only work while the USB cable is plugged in. Seeing as it is unlikely for the need to connect over the network while being close enough to safely pluck in the USB cable, the use of the USB cable in conjunction with the network connection has not been tested.

The steps listed are as follows:

1. Download and installation
2. Connecting over network
3. Connecting over wireless
4. Exiting the application
5. Downloading the software:
   1. Navigate to the location of the installer (currently U:\Downloads & Installers).
   2. download ‘Manchester Projectors IEU\_Lite\_v114.exe.ebstjzu.partial’.
   3. Navigate to the location you downloaded the file to.
   4. Rename the file to: ‘Manchester Projectors IEU\_Lite\_v114.exe’.
      1. If that does not work, go to: Control Panel > Folder Options > View.
      2. Uncheck the option 'Hide file extensions from known file types'.
      3. Try again.
   5. Run the file and when prompted; click Accept.
6. Connecting via Wired network:
   1. Switch the projector to the network input mode.
   2. Run the program: 'Image Express Utility Lite'.
   3. Select the option "Realtek PCIe FE Family Controller" under the name column and click OK.
      1. To find the name of you network adapter go to: Control Panel > Network and Sharing Centre.
      2. Click on ‘Local Area Connection’.
      3. Select Properties (You may need Administrative permissions.
      4. The content of the ‘Connect using’ field is the name of the network port you need to select.
   4. Select the projector and click Connect.
7. Connecting via Wireless network:
   1. Switch the projector to the network input mode.
   2. On the projector select 'menue > Setup > Wireless Connection > Profile > Easy Connection > Yes.
   3. Run the program: 'Image Express Utility Lite'.
   4. Select the option 'Intel(R) Centrino(R) Wireless-N 1030 #2' under the name column that is not of type ‘Easy Connection’ and and click Ok.
      1. To find the name of you network adapter go to: Control Panel > Network and Sharing Centre.
      2. Click on the Wireless network connection you wish to use.
      3. Select Properties (You may need Administrative permissions.
      4. The content of the ‘Connect using’ field is the name of the network port you need to select.
   5. Select the Projector and click Connect.
8. Exiting the connection:
   1. Select the power button on the grey toolbar that appears in the top middle of the screen.
   2. Select Exit.
   3. (Optional) Check the option to turn off the projectors power.
   4. Select OK.